**Assignment**

|  |  |
| --- | --- |
| **Name** | **AHAHAHAHAHAHAHAAAASASAHAH** |
| **Lecturer** |  |
| **Date of issue** |  |
| **Due date** |  |

***Complete the attached problems.***


***You must show formulae used to calculate answers.***

***You must draw the phasor diagrams.***

***You must show all answers with correct units of measurement.***


***WARNING CONTAINS ANSWERS***

|  |
| --- |
| ***f = 100Hz*** |
| ***Va = 230v*** |
| ***C = 3.3uF*** |
| ***L = 2.5H*** |
| ***R = 1800Ω*** |

******


|  |  |
| --- | --- |
| XL = = = 1.57kΩ | |
| Xc = 1/ = 1/ 2 = 482Ω | |
| XT = XL ~ XC = 1570 – 482 = 1.088kΩ | |
| Draw phasor diagram. | |
| Z = = = 2.1kΩ | Alternate method using polar to rectangular conversion function. |
| IT = = = 0.110A (110mA) | Z = Pol(1800,1088 = 2.1kΩ  Phase angle = RCL “F” = 31.150 |
| VR = I x R = 0.110 x 1800 = 198V | All other values calculated as per previous method |
| VL = I x XL = 0.110 x 1570 = 173V |  |
| Vc = I x XC = 0.110 x 482 = 53V |  |
| Phase angle = tan-1 = tan-1  = -31.150 |  |

|  |
| --- |
| ***f = 50Hz*** |
| ***Va = 230v*** |
| ***C = 68uF*** |
| ***L = 82mH*** |
| ***R = 32 Ω*** |

******


|  |  |
| --- | --- |
| XL = = = 26Ω | |
| Xc = 1/ = 1/ 2 = 47Ω | |
| X = XL ~ XC = 47 – 26 = 21Ω | |
| Draw phasor diagram | |
| Z = = = 38Ω | Alternate method using polar to rectangular conversion function. |
| IT = = = 6.05A | Z = Pol(32,21 = 38Ω  Phase angle = RCL “F” = - 33.270 |
| VR = I x R = 6.05 x 32 = 194V | All other values calculated as per previous method |
| VL = I x XL = 0.110 x 26 = 157V | Ɵ |
| Vc = I x XC = 0.110 x 47 = 284V |  |
| Phase angle = tan-1 = tan-1  = -33.270 |  |

|  |
| --- |
| ***f = 1kHz*** |
| ***Va = 230V*** |
| ***C = 6.3uF*** |
| ***L = 3mH*** |
| ***R = 35Ω*** |

******


|  |  |
| --- | --- |
| XL = = = 19Ω | |
| Xc = 1/ = 1/ 2 = 25Ω | |
| X = XL ~ XC = 25 – 19 = 6Ω | |
| Draw phasor diagram | |
| Z = = = 35.5Ω | Alternate method using polar to rectangular conversion function. |
| IT = = = 6.48A | Z = Pol(35,6 = 35.5Ω  Phase angle = RCL “F” = - 9.730 |
| VR = I x R = 6.48 x 35 = 227V | All other values calculated as per previous method |
| VL = I x XL = 6.48 x 19 = 123V |  |
| Vc = I x XC = 6.48 x 25 = 162V |  |
| Phase angle = tan-1 = tan-1  = -9.730 |  |

|  |
| --- |
| ***f = 50Hz*** |
| ***Va = 240V*** |
| ***C = 2.2uF*** |
| ***L = 2.7H*** |
| ***R = 820Ω*** |

******

|  |  |
| --- | --- |
| XL = = = 848Ω | |
| Xc = 1/ = 1/ 2 = 1.447kΩ | |
| X = XL ~ XC = 1447 – 848 = 599Ω | |
| Draw phasor diagram | |
| Z = = = 1015Ω | Alternate method using polar to rectangular conversion function. |
| IT = = = 0.236A (236mA) | Z = Pol(820,599 = 1.015kΩ  Phase angle = RCL “F” = - 36.150 |
| VR = I x R = 0.236 x 820 = 194V | All other values calculated as per previous method |
| VL = I x XL = 0.236 x 848 = 200V |  |
| Vc = I x XC = 0.236 x 1447 = 341V |  |
| Phase angle = tan-1 = tan-1  = -36.150 |  |

|  |
| --- |
| ***f = 1.5kHz*** |
| ***Va =230V*** |
| ***C = 15nF*** |
| ***L = 330mH*** |
| ***R = 3.3kΩ*** |

******

|  |  |
| --- | --- |
| XL = = = 3.11kΩ | |
| Xc = 1/ = 1/ 2 = 7.07kΩ | |
| X = XL ~ XC = 1447 – 848 = 3.96kΩ | |
| Draw phasor diagram | |
| Z = = = 5.155kΩ | Alternate method using polar to rectangular conversion function. |
| IT = = = 0.045A (45mA) | Z = Pol(3300,3960 =5.155kΩ  Phase angle = RCL “F” = - 50.190 |
| VR = I x R = 0.045 x 3300 = 148.5V | All other values calculated as per previous method |
| VL = I x XL = 0.045 x 3110 = 140V |  |
| Vc = I x XC = 0.045 x 7070 = 318V |  |
| Phase angle = tan-1 = tan-1  = -50.190 |  |