**Colour Resistor Code**

**ANSWERS**

1. **(a) 650k, +/- 10%**

 **(b) 158R, +/- 1%**

 **(c) 920R, +/- 5%**

 **(d) 24k, +/- 5%**

 **(e) 34k5, +/- 2%**

 **(f) 72k, +/- 5%**

 **(g) 89M6, +/- 1%**

**2. (a) Red, White, Red, Gold**

 **(b) Yellow, Violet, Gold, Silver**

 **(c) Orange, White, Green, Black, Red**

 **(d) Brown, Red, Green, Gold**

 **(e) Yellow, Violet, Yellow, Brown or Yellow, Violet, Black, Orange, Brown**

 **(f) Green, Blue, Grey, Orange, Brown**

 **(g) Blue, Grey, Gold, Silver**

 **(h) Grey, Red, Silver, Gold**

 **(I) Orange, Orange, Gold, Red**

 **(j) Brown, Red, Red, Red, Brown**