**Gold Hill Radio Watch**

**Dual Display Guide**



The Wouxun KG-935G radio has “dual display” functionality, which allows for monitoring two channels/frequencies at the same time.

**Area A**

**Area B**

The upper display is “Area A” and lower is “Area B.”

When the dual display is off, the inactive display will have the text “KG-935G.” The inactive display can be in either Area A or B.

**To turn the dual display on or off** use the [TDR] key (which stands for True Dual Receive) on the keypad.

[Band] – Switches which area is primary (with short press).

[TDR] – True Dual Receive. Turns Dual Display on and off.

**The primary display area** is larger, occupying about two-thirds of the screen and has a red “MAIN” icon to the right of the channel or frequency.[[1]](#footnote-1) The channel/frequency displayed in the primary area is the one that will be affected by operations you perform—like transmitting or changing the channel.



**The secondary display area** is the smaller area. Its channel/frequency is just being monitored.

**Primary**- bigger,

- “Main” icon

**To switch the primary area** (with Dual Display on), press the [BAND] key on the keypad. Note, if you press it for too long (2 seconds), it will activate NOAA Weather instead.

**Secondary**

**Exercises:**

In this example, the Banner repeater is primary. If you wanted to talk on Channel 4, you’d need to push the [Band] button to make Channel 4 primary.

1. **Switching between Banner and Channel 4 as primary.**

a. Starting with Dual Display off, then set up the radio to   
have Channel 4 as primary and Banner as secondary.

b. Then switch to Banner as primary (making it possible to transmit to the Banner repeater).

c. Then switch back to Channel 4 as primary.

2. **Turning NOAA Weather on and off.**

a. With Dual Display on, press the [Band] key for 2 seconds, activating the NOAA weather frequency in Area A.

b. Press the [Band] key for 2 seconds again to revert to the previous channel.

1. The Main icon displays only if the radio is in Channel Name mode, which is the mode we use. [↑](#footnote-ref-1)